## lifcl17 pins for testing based on breakout board
set_property PACKAGE_PIN 55 [get_ports clk]
set_property PACKAGE_PIN 57 [get_ports rst]
set_property PACKAGE_PIN 56 [get_ports io_led[4]]
set_property PACKAGE_PIN 59 [get_ports io_led[5]]
set_property PACKAGE_PIN 60 [get_ports io_led[6]]
set_property PACKAGE_PIN 61 [get_ports io_led[7]]

set_property IOSTANDARD LVCMOS33 [get_ports clk]
set_property IOSTANDARD LVCMOS33 [get_ports rst]
set_property IOSTANDARD LVCMOS33 [get_ports io_led[4]]
set_property IOSTANDARD LVCMOS33 [get_ports io_led[5]]
set_property IOSTANDARD LVCMOS33 [get_ports io_led[6]]
set_property IOSTANDARD LVCMOS33 [get_ports io_led[7]]
